(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "BQ25703ARSNR" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 2.54 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Value" "BQ25703ARSNR" (id 1) (at 0 0 0)
      (effects (font (size 1.524 1.524)))
    )
    (property "Footprint" "RSN0032B" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/gpn/bq25703a" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "ki_keywords" "BQ25703ARSNR" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_locked" "" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_fp_filters" "RSN0032B" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BQ25703ARSNR_0_1"
      (polyline
        (pts
          (xy -17.78 -50.8)
          (xy 17.78 -50.8)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.78 -50.8)
          (xy 17.78 50.8)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 17.78 50.8)
          (xy -17.78 50.8)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -17.78 50.8)
          (xy -17.78 -50.8)
        )
        (stroke (width 0.2032) (type default) (color 0 0 0 0))
        (fill (type none))
      )
      (pin power_in line (at -22.86 25.4 0) (length 5.08)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 20.32 0) (length 5.08)
        (name "ACN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 15.24 0) (length 5.08)
        (name "ACP" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -22.86 -30.48 0) (length 5.08)
        (name "CHRG_OK" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -35.56 0) (length 5.08)
        (name "EN_OTG" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 0 0) (length 5.08)
        (name "ILIM_HIZ" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 10.16 0) (length 5.08)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -25.4 180) (length 5.08)
        (name "IADPT" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -30.48 180) (length 5.08)
        (name "IBAT" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 -35.56 180) (length 5.08)
        (name "PSYS" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -22.86 -15.24 0) (length 5.08)
        (name "PROCHOT_N" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -25.4 0) (length 5.08)
        (name "SDA" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -20.32 0) (length 5.08)
        (name "SCL" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -45.72 0) (length 5.08)
        (name "CMPIN" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin open_collector line (at -22.86 -40.64 0) (length 5.08)
        (name "CMPOUT" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -22.86 -7.62 0) (length 5.08)
        (name "COMP1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -7.62 180) (length 5.08)
        (name "COMP2" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -17.78 180) (length 5.08)
        (name "CELL_BATPRES" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 10.16 180) (length 5.08)
        (name "SRN" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 15.24 180) (length 5.08)
        (name "SRP" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 20.32 180) (length 5.08)
        (name "BATDRV_N" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 25.4 180) (length 5.08)
        (name "VSYS" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 40.64 180) (length 5.08)
        (name "SW2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 30.48 180) (length 5.08)
        (name "HIDRV2" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 45.72 180) (length 5.08)
        (name "BTST2" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 22.86 35.56 180) (length 5.08)
        (name "LODRV2" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -40.64 180) (length 5.08)
        (name "PGND" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 2.54 180) (length 5.08)
        (name "REGN" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -22.86 35.56 0) (length 5.08)
        (name "LODRV1" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 45.72 0) (length 5.08)
        (name "BTST1" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -22.86 30.48 0) (length 5.08)
        (name "HIDRV1" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -22.86 40.64 0) (length 5.08)
        (name "SW1" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -45.72 180) (length 5.08)
        (name "PAD" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
    )
  )
)

