
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "BQ25703ARSNR" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -10.16 5.08 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "BQ25703ARSNR" (id 1) (at -33.02 -10.16 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "BQ25703ARSNR:BQ25703A_QFN-32" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Texas Instruments" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            I2C 1-4 cell NVDC Buck-Boost battery charge controller with system power monitor & processor\n                        \n" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "WQFN-32 Texas Instruments" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/BQ25703ARSNR/Texas+Instruments/view-part/?ref=snap" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "BQ25703ARSNR" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/BQ25703ARSNR/Texas+Instruments/view-part/?ref=eda" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "BQ25703ARSNR_0_0"
      (rectangle (start -45.72 -45.72) (end 45.72 45.72)
        (stroke (width 0.508)) (fill (type background))
      )
      (pin bidirectional line (at -35.56 50.8 270.0) (length 5.08)
        (name "HIDRV1"
          (effects (font (size 1.016 1.016)))
        )
        (number "31"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -25.4 50.8 270.0) (length 5.08)
        (name "LODRV1"
          (effects (font (size 1.016 1.016)))
        )
        (number "29"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 50.8 270.0) (length 5.08)
        (name "SW1"
          (effects (font (size 1.016 1.016)))
        )
        (number "32"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -5.08 50.8 270.0) (length 5.08)
        (name "BTST1"
          (effects (font (size 1.016 1.016)))
        )
        (number "30"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 5.08 50.8 270.0) (length 5.08)
        (name "BTST2"
          (effects (font (size 1.016 1.016)))
        )
        (number "25"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 50.8 270.0) (length 5.08)
        (name "SW2"
          (effects (font (size 1.016 1.016)))
        )
        (number "23"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 25.4 50.8 270.0) (length 5.08)
        (name "LODRV2"
          (effects (font (size 1.016 1.016)))
        )
        (number "26"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 35.56 50.8 270.0) (length 5.08)
        (name "HIDRV2"
          (effects (font (size 1.016 1.016)))
        )
        (number "24"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 35.56 0) (length 5.08)
        (name "VBUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 25.4 0) (length 5.08)
        (name "ACN"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 15.24 0) (length 5.08)
        (name "ACP"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 5.08 0) (length 5.08)
        (name "VDDA"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 -5.08 0) (length 5.08)
        (name "ILIM_HIZ"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 -15.24 0) (length 5.08)
        (name "COMP1"
          (effects (font (size 1.016 1.016)))
        )
        (number "16"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 -25.4 0) (length 5.08)
        (name "COMP2"
          (effects (font (size 1.016 1.016)))
        )
        (number "17"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -50.8 -35.56 0) (length 5.08)
        (name "~{PROCHOT}"
          (effects (font (size 1.016 1.016)))
        )
        (number "11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -35.56 -50.8 90.0) (length 5.08)
        (name "SDA"
          (effects (font (size 1.016 1.016)))
        )
        (number "12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -25.4 -50.8 90.0) (length 5.08)
        (name "SCL"
          (effects (font (size 1.016 1.016)))
        )
        (number "13"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 -50.8 90.0) (length 5.08)
        (name "CHRG_OK"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -5.08 -50.8 90.0) (length 5.08)
        (name "EN_OTG"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 5.08 -50.8 90.0) (length 5.08)
        (name "CMPOUT"
          (effects (font (size 1.016 1.016)))
        )
        (number "15"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 -50.8 90.0) (length 5.08)
        (name "CMPIN"
          (effects (font (size 1.016 1.016)))
        )
        (number "14"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 35.56 -50.8 90.0) (length 5.08)
        (name "IBAT"
          (effects (font (size 1.016 1.016)))
        )
        (number "9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -35.56 180.0) (length 5.08)
        (name "IADPT"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -25.4 180.0) (length 5.08)
        (name "CELL_BATPRESZ"
          (effects (font (size 1.016 1.016)))
        )
        (number "18"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08)
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "27"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "GND"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "GND1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -15.24 180.0) (length 5.08) hide
        (name "PGND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P$9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 -5.08 180.0) (length 5.08)
        (name "REGN"
          (effects (font (size 1.016 1.016)))
        )
        (number "28"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 5.08 180.0) (length 5.08)
        (name "SRN"
          (effects (font (size 1.016 1.016)))
        )
        (number "19"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 15.24 180.0) (length 5.08)
        (name "SRP"
          (effects (font (size 1.016 1.016)))
        )
        (number "20"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 25.4 180.0) (length 5.08)
        (name "~{BATDRV}"
          (effects (font (size 1.016 1.016)))
        )
        (number "21"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 50.8 35.56 180.0) (length 5.08)
        (name "VSYS"
          (effects (font (size 1.016 1.016)))
        )
        (number "22"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 25.4 -50.8 90.0) (length 5.08)
        (name "PSYS"
          (effects (font (size 1.016 1.016)))
        )
        (number "10"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)